



This guide provides information on the daily use of the DP-330/330L printer.   
For additional information, please refer to the DP-330/330L User Guide.


**DP-330/330L**


**Quick Start Guide**

****


**Printer features Media**

*Tear paper towards back of printer*





Paper Door



Paper door release button


NOTE:   
When using 2” paper, install spacer.


Power Port


Control Panel

USB Data Port

Press Paper door release button to open the paper compartment door. Pull small leader of paper out and close paper door. “ Clicks” when properly closed.

****

******Performing a Printer Self-Test Battery**



Loosen hand strap (not pictured) to access battery door.  
  
Rotate knob 180o  to unlock battery door.  
  
Drop in battery.


Close battery door and rotate knob 180o to lock.




With power on, press the paper feed button for three seconds.

Press button to see battery charge level.  
4LED 100% charge  
3LED 75%  
2LED 50%  
1LED 25%


**Disposal**  
Please dispose the batteries separately and free of cost at your sales agency or the designated local collecting points.  
Therefore please consider the national recycling standards!  
Disassembly and removal of the batteries are described in the User Guide.



**DP-330/330L Quick Start Guide**

**Control Panel indicators**

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Status | Power light | Charge light | Caution light | Buzz |
| Buffer has data | Green light-twinkle | Change according to power |  |  |
| Buffer is empty | Green light-on |  |  |
| Standby | Change according to the Buffer status | Off | / |
| Setting mode  (Config tools mode) | Orange light-on | Off | / |
| Open cover/paper out | Change according to the Buffer status | Red light-on | Buzz/  2 seconds |
| Paper on the peeler | Orange light-on | / |
| Black mark/label position is error | Red light-twinkle | / |
| Print head is overheating | Green light-breathing light | / |
| Print head is ultracold temperature | Red light is on | Green light-breathing light | / |
| EEPROM is error | Red light is on | Red light-on | / |
| Battery power read error | Change according to the Buffer status | Off | Green light-on | / |
| Power saving mode | Green light-breathing light | Off | Off | / |
| Download mode | At the same time, the three lights green-red alternating cycle flicker: Green-red-green-red. | | | / |
| Loading | At the same time, the three lights flicker with orange color. | | | / |




**Install the Config Tool**


3. When the progress bar is full, the right picture will be shown, click “Finish” to complete the installation.

2. Click “next”, enter installation interface.

1. Download the latest setup tool

“Config Tool” from official website .



**Dascom Representatives**

Americas Dascom Americas Corp 34 Lakeview Court Verona, VA 24482, USA Phone: +1 (877) 434 1377  
UK DASCOM GB Ltd Hart House, Priestley Road Basingstoke, Hampshire, RG24 9PU Phone: +44 (0) 1256 481481  
Germany DASCOM Europe GmbH Heuweg 3 D-89079 Ulm Phone: +49 (0) 731 2075 0  
France DASCOM Europe GmbH 117 Avenue Victor Hugo 92100 Boulogne-Billancourt Phone: +33 (1)73 02 51 98  
Singapore (AP) DASCOM AP Pte Ltd 2 Jurong East Street 21 #05-42, IMM Building, Singapore 609601 Phone: +65 6760 8833

21.511.929.0040R